**red>100&&blue>100&&green>100**

**Sensor part RGB LED blinks and Get the analog values from LDR**

**Blue LED blink**

**Green LED blink**

**Red LED blink**

**Inset color.**

**blue>red&&blue>green&&blue>50**

**green>red&&green>blue&&green>100**

**red>green&&red>blue&&50<red**

**White LED blink**